**ADDENDUM NO. Fuel Pump #1**

*Prepared by:* Brad Hansen, Hoffman Estates Park District

*Date Issued*: April 11, 2017

*Project:*  **Supply and Install new fuel pumps**

NOTE: The following changes are hereby made to the contract documents and insofar as the original contract Documents are inconsistent therewith, the changes herein shall govern. All Bidders shall acknowledge this addendum by inserting its number and date on their bid form.

*Items included in this addendum:*

**Options to include in Base Price have been altered to specify (SS) Super Stainless Steel – all panels each dispenser. See highlighted in green on new Specifications Sheet below. (Please scroll down)**

**End of Addendum Fuel Pump #1**

**SPECIFICATIONS**

**The Hoffman Estates Park District parks maintenance facility installation of new Bennett fuel pumps**

1. **Secure State Fire Marshal (OSFM) and village Permits if required**
2. **Remove (2) existing fuel dispensing pumps and disposal of**.
3. **Install (2) new OPW70 suction check valves onto (2) pipe risers at island including strut bracing to island.**
4. **Provide and install on island (2) each new Bennett # 3112SNS-5**:
* Commercial Suction Pump.
* Mechanical register.
* Resettable totalizer.
* Single product.
* Low hose.
* Dual hose.
* Side-mount nozzles.
* Product placards. One dispenser will be for Unleaded Fuel and the second for Diesel Fuel.
* Freight to site.

**Options to include in base price:**

* + (P10) 10:1 gallon pulser, per hose.
	+ (SS) Super Stainless Steel - all panels each dispenser.

**Supply & install hanging hardware onto new dispensers as follows:**

* (4) OPW 80” high hose retractors
* (4) ¾” hose clamps,
* (4) ¾” X 10’ hardwall hoses,
* (4) 9” hardwall whip hoses
* (2) new OPW 11 A leaded nozzles for diesel
* (2) OPW 11 A nozzles for gasoline
* (4) OPWA 241 TPS Swivels
* (4) OPW 66REC re-connectable breakaways.
1. **Place dispensers on Fuel Island, anchor and make pipe and electric connections including connecting to Petro Vend fuel management system. All electric is figured to be in good, useable condition. Addition of any junction boxes under dispenser, if required, is to be included.**
2. **Test, purge, calibrate and commission new dispensers.**
3. **Submit warranty paperwork**.
4. **Train owner on use of new equipment**.
5. **Coordinate inspections if required.**

**My contact information to set up an on-site appointment is**

Brad Hansen

Mechanic Supervisor

847-285-5470

bhansen@heparks.org